4.6 GEMSQRAW: UTILITIES

Utility Programs

wordfig | Save the last plot in a file gemsqraw.cgm suitable for inclusion in a Word document.
las | Save the last plot in a postscript file genie.ps and send it to the laser printer - if you give a laser printer number as a parameter (e.g. type LAS 2) then this will be used to determine which printer to use, otherwise the plot will be sent to the printer in the GEM cabin.
nspec() | Gives the number of spectra for the specified run e.g. type printn nspec(5462).
head() | Gives the header for the specified run e.g. type printn head(7422).
uamp() | Gives the number of microAmp-hours for the specified run e.g. type printn uamp(220).
readsum() | Read an ATLAS file (a .SUM file by default) into an OpenGenie WorkspaceArray e.g. type vdata=readsum(1170,"SMO")
wd | Display all elements of a WorkspaceArray on a single frame graph. e.g. type wd bank.
wp | Overplot all elements of a WorkspaceArray on a graph produced by wd. e.g. type wp sio2.

Last updated on 26 Feb 2003 by Alex Hannon (a.c.hannon@rl.ac.uk)